%%{
/*
 * Copyright (c) 2018-2019, Texas Instruments Incorporated - http://www.ti.com
 * All rights reserved.
 *
 * Redistribution and use in source and binary forms, with or without
 * modification, are permitted provided that the following conditions
 * are met:
 *
 * *  Redistributions of source code must retain the above copyright
 *    notice, this list of conditions and the following disclaimer.
 *
 * *  Redistributions in binary form must reproduce the above copyright
 *    notice, this list of conditions and the following disclaimer in the
 *    documentation and/or other materials provided with the distribution.
 *
 * *  Neither the name of Texas Instruments Incorporated nor the names of
 *    its contributors may be used to endorse or promote products derived
 *    from this software without specific prior written permission.
 *
 * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
 * AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
 * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
 * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
 * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
 * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
 * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS;
 * OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY,
 * WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR
 * OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE,
 * EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
 *
 */

/*
 *  ======== VREF.Board.c.xdt ========
 */

    let VREF = args[0];
    let content = args[1];

    let Common = system.getScript("/ti/driverlib/Common.js");

    /* shorthand names for some common references in template below */
    let instances = VREF.$static;
    if (instances.length == 0) return;

/*
 * Standard Trampoline:
 * In order to preserve spacing, it is important to also set the boolean
 * values in the templates object based on whether that condition should
 * produce any code
 * Example:
 * templates: {
 *       boardc: "/ti/driverlib/comp/COMP.Board.c.xdt",
 *       boardh: "/ti/driverlib/comp/COMP.Board.h.xdt",
 *       Call: true,
 *       Reset: false,
 *       Power: true,
 *       GPIO: false,
 *       Function: true
 * },
 */


    switch(content){
        case "Call":
            printCall();
            break;
        case "Reset":
            printReset();
            break;
        case "Power":
            printPower();
            break;
        case "GPIO":
            printGPIO();
            break;
        case "Function":
            printFunction();
            break;
        default:
            /* do nothing */
            return;
            break;
    }
%%}
%
% function printCall(){
    SYSCFG_DL_VREF_init();
% }
%
% function printReset(){
    DL_VREF_reset(VREF);
%
% }
% function printPower(){
%       /* another possibility depending on the driver */
    DL_VREF_enablePower(VREF);
% }
%
% function printGPIO(){
%       let inst = instances;
%       /* all of these are defined in the header */
%       let gpioStr = "GPIO_VREF";
%       // No need to initialize GPIOs for Analog functionality
%       /* Peripheral GPIO Configuration */
%       let initIOMux = Common.getGPIOConfigBoardC(inst);
%       /* Check if generating empty code */
%       if (/\S/.test(initIOMux)) {
    `initIOMux`
%       }
% }
%
% /* Main Function */
% function printFunction(){
%   let inst = instances;

%   if (inst.advClockConfigEnable == true) {
static const DL_VREF_ClockConfig gVREFClockConfig = {
    .clockSel = `inst.advClkSrc`,
    .divideRatio = `inst.advClkDiv`,
};
%   } // if (inst.advClockConfigEnable == true)
static const DL_VREF_Config gVREFConfig = {
% let vrefEn = ((inst.basicMode.includes("DL_VREF_ENABLE_ENABLE"))?"DL_VREF_ENABLE_ENABLE":"DL_VREF_ENABLE_DISABLE")
    .vrefEnable     = `vrefEn`,
%   if (inst.basicMode.includes("DL_VREF_ENABLE_ENABLE")){
%   // Internal mode
    .bufConfig      = `inst.basicIntVolt`,
%   } else{
%   // External mode
    .bufConfig      = DL_VREF_BUFCONFIG_OUTPUT_2_5V,
%   }
%   if (inst.advSHEnable == true){
    .shModeEnable   = DL_VREF_SHMODE_ENABLE,
    .holdCycleCount = `inst.advSHSample`,
    .shCycleCount   = `inst.advSHHold`,
%   } else {
    .shModeEnable   = DL_VREF_SHMODE_DISABLE,
    .holdCycleCount = DL_VREF_HOLD_MIN,
    .shCycleCount   = DL_VREF_SH_MIN,
%   }
};

SYSCONFIG_WEAK void SYSCFG_DL_VREF_init(void) {
%   if (inst.advClockConfigEnable == true) {
    DL_VREF_setClockConfig(VREF,
        (DL_VREF_ClockConfig *) &gVREFClockConfig);
%   }
    DL_VREF_configReference(VREF,
        (DL_VREF_Config *) &gVREFConfig);
%
% /* After writing VREF_EN to '1', wait for fix time instead of relying on VREF_READY status. */
% if (inst.checkVREFReady) {
    delay_cycles(VREF_READY_DELAY);
%%{ // TODO: [(H) JAN] this code is likely to be removed in favor of the delay (MSPSWSDK-2038).
    // while (DL_VREF_CTL1_READY_NOTRDY == DL_VREF_getStatus(VREF))
    //     ;
%%}
% }
}

% } // printFunction()
