# Readme

## Example Summary

Empty project using DriverLib. This example shows a basic empty project using DriverLib with just main file and SysConfig initialization.

## Peripherals & Pin Assignments

Peripheral | Pin | Function
--- | --- | ---
SYSCTL |  |
DEBUGSS | PA20 | Debug Clock
DEBUGSS | PA19 | Debug Data In Out

## BoosterPacks, Board Resources & Jumper Settings

Visit LP_MSPM0L1306 for LaunchPad information, including user guide and hardware files.

Pin | Peripheral | Function | LaunchPad Pin | LaunchPad Settings
--- | --- | --- | --- | ---
PA20 | DEBUGSS | SWCLK | J2_13 | PA20 is used by SWD during debugging `J101 15:16 ON` Connect to XDS-110 SWCLK while debugging `J101 15:16 OFF` Disconnect from XDS-110 SWCLK if using pin in application
PA19 | DEBUGSS | SWDIO | J2_17 | PA19 is used by SWD during debugging `J101 13:14 ON` Connect to XDS-110 SWDIO while debugging `J101 13:14 OFF` Disconnect from XDS-110 SWDIO if using pin in application

### Device Migration Recommendations

This project was developed for a superset device included in the LP_MSPM0L1306 LaunchPad. Please visit the CCS User’s Guide for information about migrating to other MSPM0 devices.

### Low-Power Recommendations

TI recommends to terminate unused pins by setting the corresponding functions to GPIO and configure the pins to output low or input with internal pullup/pulldown resistor.

SysConfig allows developers to easily configure unused pins by selecting Board→Configure Unused Pins.

For more information about jumper configuration to achieve low-power using the MSPM0 LaunchPad, please visit the LP-MSPM0L1306 User’s Guide.

## Example Usage

Compile, load and run the example.