%%{
/*
 * Copyright (c) 2022, Texas Instruments Incorporated - http://www.ti.com
 * All rights reserved.
 *
 * Redistribution and use in source and binary forms, with or without
 * modification, are permitted provided that the following conditions
 * are met:
 *
 * *  Redistributions of source code must retain the above copyright
 *    notice, this list of conditions and the following disclaimer.
 *
 * *  Redistributions in binary form must reproduce the above copyright
 *    notice, this list of conditions and the following disclaimer in the
 *    documentation and/or other materials provided with the distribution.
 *
 * *  Neither the name of Texas Instruments Incorporated nor the names of
 *    its contributors may be used to endorse or promote products derived
 *    from this software without specific prior written permission.
 *
 * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
 * AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO,
 * THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR
 * PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR
 * CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL,
 * EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
 * PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS;
 * OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY,
 * WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR
 * OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE,
 * EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
 *
 */

/*
 *  ======== oscillator.Board.c.xdt ========
 */

    let Common = system.getScript("/ti/driverlib/Common.js");

    let mod = system.modules["/ti/clockTree/oscillator.js"];
    let content = args[0];

    let sysoscInst = _.find(mod.$instances, ['$name', 'SYSOSC']);
    let lfoscInst = _.find(mod.$instances, ['$name', 'LFOSC']);

    if(_.isUndefined(sysoscInst) || _.isUndefined(lfoscInst)) {
        throw 'Not all oscillator elements are defined appropriately';
    }
%%}
%
%
% if(!sysoscInst.disableSYSOSC && sysoscInst.enableROSC){
% /* ROSC pins */
%       let roscPinName = "roscPin";
%       let roscPackagePin = sysoscInst.peripheral[roscPinName].$solution.packagePinName;
%       let roscPinCM = Common.getPinCM(roscPackagePin,sysoscInst,"ROSC");
%       let roscGpioName = system.deviceData.devicePins[roscPackagePin].mux.muxSetting[0].peripheralPin.peripheralName;
%       let roscPort = Common.getGPIOPortMultiPad(roscPackagePin,sysoscInst,"ROSC");
%       let roscGpioPin = Common.getGPIONumberMultiPad(roscPackagePin,sysoscInst,"ROSC");
% let roscPortStr = "#define GPIO_ROSC_PORT";
`roscPortStr.padEnd(40," ")+roscPort.padStart(40, " ")`
% let roscPinStr = "#define GPIO_ROSC_PIN";
% let roscPinStr2 = "DL_GPIO_PIN_"+roscGpioPin;
`roscPinStr.padEnd(40," ")+roscPinStr2.padStart(40," ")`
% let roscIOmuxStr = "#define GPIO_ROSC_IOMUX";
% let roscIOmuxStr2 = "(IOMUX_PINCM"+roscPinCM.toString()+")";
`roscIOmuxStr.padEnd(40," ")+roscIOmuxStr2.padStart(40," ")`
% }
